{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Initial","How to Use","Selection Tool"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Initial","index":0,"n_rows":58,"n_cols":23,"rows_kept":58,"cut":false,"hidden":true,"merged":[[0,13,0,15],[0,0,1,0],[0,8,0,10],[0,11,0,12],[0,1,0,4],[0,5,0,7]]}
["Tool","Data Needed",null,null,null,"Subsurface/Surface",null,null,"Data Quality",null,null,"Data Collection",null,"Additional Info"]
[null,"Geology","Hydrogeology","Chemistry","Topography","Consolidated /Bedrock  ","Unconsolidated","Surface","Quantitative","Semi-Quantitative","Qualitative","Invasive","Non-Invasive","Summary Table","Checklist","Case Study"]
["Direct Sensing",null,null,null,null,null,null,null,null,null,null,null,null,"DS_ST","DS_CL",null,null,3,null,"https://asct-1.itrcweb.org/3-direct-sensing/ ","https://asct-1.itrcweb.org/tables_checklists/asct_direct_sensing_tool_summary_table.pdf","https://asct-1.itrcweb.org/tables_checklists/asct_direct_sensing_checklists.pdf"]
["Membrane Interface Probe (MIP)",null,null,"X",null,"X1","X",null,null,"X",null,"X",null,null,null,"9.1 (9.2)",null,3.2,9.1,"https://asct-1.itrcweb.org/3-2-membrane-interface-probe/",null,null,"https://asct-1.itrcweb.org/9-1-mip-boring-data-allow-on-site-decisions-to-fill-data-gaps-and-reduce-uncertainty-during-triad-approach-evaluation-at-five-south-dakota-sites/"]
["Optical Image Profiler (OIP-UV, OIP-G)",null,null,"X",null,"X1","X",null,null,"X",null,"X",null,null,null,9.3000000000000007,null,3.3,9.3000000000000007,"https://asct-1.itrcweb.org/3-3-optical-image-profiler/",null,null,"https://asct-1.itrcweb.org/9-3-oip-green-probe-delineates-extent-of-coal-tar-napl-at-a-former-gas-manufacturing-plant-in-kansas/"]
["Laser Induced Fluoresence (LIF)",null,null,"X",null,"X1","X",null,null,"X",null,"X",null,null,null,"9.4 (9.5/9.6)",null,3.4,9.4,"https://asct-1.itrcweb.org/3-4-laser-induced-fluorescence/",null,null,"https://asct-1.itrcweb.org/9-4-lif-survey-with-uovost-provides-more-accurate-representation-of-lnapl-plume-at-a-former-bulk-petroleum-storage-facility-in-new-hampshire/"]
["Cone Penetrometer Testing (CPT)","X","X",null,null,"X1","X",null,"X",null,null,"X",null,null,null,9.6999999999999993,null,3.5,9.6999999999999993,"https://asct-1.itrcweb.org/3-5-cone-penetrometer-testing/",null,null,"https://asct-1.itrcweb.org/9-7-cpt-borings-and-hydropunch-sampler-optimize-site-characterization-at-an-aviation-industrial-complex-in-california/"]
["Hydraulic Profiling (WaterlooAPS and HPT) ","X","X",null,null,"X1","X",null,"X","X","X","X",null,null,null,9.8000000000000007,null,3.6,9.8000000000000007,"https://asct-1.itrcweb.org/3-6-hydraulic-and-groundwater-profiling-tools/",null,null,"https://asct-1.itrcweb.org/9-8-waterloo-aps-cpt-and-lif-data-update-csm-and-help-optimize-selected-remedy-at-a-former-refinery-in-oklahoma/"]
["Electrical Conductivity (EC)","X",null,"X",null,"X1","X",null,null,"X","X","X",null,null,null,null,null,3.7,null,"https://asct-1.itrcweb.org/3-7-electrical-conductivity-ec-probe/"]
["Flexible Underground Technology (FLUTe)",null,"X","X",null,"X",null,null,"X","X","X","X",null,null,null,null,null,3.8,null,"https://asct-1.itrcweb.org/3-8-flexible-liners/"]
["Borehole Geophysics",null,null,null,null,null,null,null,null,null,null,null,null,"BG_ST","BG_CL",null,null,4,null,"https://asct-1.itrcweb.org/4-borehole-geophysics/","https://asct-1.itrcweb.org/tables_checklists/asct_borehole_geophysics_tool_summary_table.pdf","https://asct-1.itrcweb.org/tables_checklists/asct_borehole_geophysics_checklists.pdf"]
["Fluid Temperature ",null,null,"X",null,null,null,null,"X",null,null,"X",null,null,null,9.9,null,4.2,9.9,"https://asct-1.itrcweb.org/4-borehole-geophysics/#4_2",null,null,"https://asct-1.itrcweb.org/9-9-conceptual-site-model-development-using-borehole-geophysics-at-the-savage-municipal-water-supply-superfund-site-in-new-hampshire/"]
["Fluid Resisitivity",null,null,"X",null,"X",null,null,null,"X",null,"X",null,null,null,9.9,null,4.3,9.9,"https://asct-1.itrcweb.org/4-borehole-geophysics/#4_3",null,null,"https://asct-1.itrcweb.org/9-9-conceptual-site-model-development-using-borehole-geophysics-at-the-savage-municipal-water-supply-superfund-site-in-new-hampshire/"]
["Mechanical Caliper ","X",null,null,null,"X",null,null,null,"X",null,"X",null,null,null,9.9,null,4.4000000000000004,9.9,"https://asct-1.itrcweb.org/4-borehole-geophysics/#4_4",null,null,"https://asct-1.itrcweb.org/9-9-conceptual-site-model-development-using-borehole-geophysics-at-the-savage-municipal-water-supply-superfund-site-in-new-hampshire/"]
["Optical Televiewer (OTV) ","X","X",null,null,"X",null,null,null,"X",null,"X",null,null,null,9.9,null,4.5,9.9,"https://asct-1.itrcweb.org/4-borehole-geophysics/#4_5",null,null,"https://asct-1.itrcweb.org/9-9-conceptual-site-model-development-using-borehole-geophysics-at-the-savage-municipal-water-supply-superfund-site-in-new-hampshire/"]
["Acoustic Televiewer (ATV) ","X","X",null,null,"X",null,null,null,"X",null,"X",null,null,null,9.9,null,4.5999999999999996,9.9,"https://asct-1.itrcweb.org/4-borehole-geophysics/#4_6",null,null,"https://asct-1.itrcweb.org/9-9-conceptual-site-model-development-using-borehole-geophysics-at-the-savage-municipal-water-supply-superfund-site-in-new-hampshire/"]
["Natural Gamma ","X",null,null,null,"X","X",null,null,"X",null,"X",null,null,null,9.9,null,4.7,9.9,"https://asct-1.itrcweb.org/4-borehole-geophysics/#4_7",null,null,"https://asct-1.itrcweb.org/9-9-conceptual-site-model-development-using-borehole-geophysics-at-the-savage-municipal-water-supply-superfund-site-in-new-hampshire/"]
["Heat Pulse Flow Meter",null,"X",null,null,null,null,null,null,"X",null,"X",null,null,null,9.9,null,"4.8.1",9.9,"https://asct-1.itrcweb.org/4-borehole-geophysics/#4_8_1",null,null,"https://asct-1.itrcweb.org/9-9-conceptual-site-model-development-using-borehole-geophysics-at-the-savage-municipal-water-supply-superfund-site-in-new-hampshire/"]
["Impeller Flowmeter","X","X",null,null,null,null,null,null,"X",null,"X",null,null,null,null,null,"4.8.2",null,"https://asct-1.itrcweb.org/4-borehole-geophysics/#4_8_2"]
["Electrical Resitivity ",null,null,"X",null,"X",null,null,null,"X",null,"X",null,null,null,9.11,null,"4.9.1",9.11,"https://asct-1.itrcweb.org/4-borehole-geophysics/#4_9_1",null,null,"https://asct-1.itrcweb.org/9-11-surface-and-borehole-geophysical-technologies-provide-data-to-pinpoint-and-characterize-karst-features-at-a-former-retail-petroleum-facility-in-kentucky/"]
["Nuclear Magnetic Resonance (NMR)",null,"X","X",null,"X","X",null,"X",null,null,"X",null,null,null,9.9,null,"4.9.2",null,"https://asct-1.itrcweb.org/4-borehole-geophysics/#4_9_2"]
["Borehole Video ","X",null,null,null,"X","X",null,null,null,"X","X",null,null,null,9.9,null,"4.9.3",null,"https://asct-1.itrcweb.org/4-borehole-geophysics/#4_9_3"]
["Surface Geophysics",null,null,null,null,null,null,null,null,null,null,null,null,"SG_ST","SG_CL",null,null,5,null,"https://asct-1.itrcweb.org/5-surface-geophysics/","https://asct-1.itrcweb.org/tables_checklists/asct_surface_geophysics_tool_summary_table.pdf","https://asct-1.itrcweb.org/tables_checklists/asct_surface_geophysics_checklists.pdf"]
["Electrical Resistivity Inaging (ERI) (Tomography (ERT)) ","X","X","X",null,"X","X",null,null,"X","X",null,"X",null,null,"9.13 (9.10/9.15)",null,5.2,9.1300000000000008,"https://asct-1.itrcweb.org/5-surface-geophysics/#5_2",null,null,"https://asct-1.itrcweb.org/9-13-resistivity-seismic-exploration-and-gpr-provide-data-to-evaluate-clay-reserves-at-a-commercially-mined-pit/"]
["Ground Penetrating Radar (GPR)","X","X",null,null,"X","X",null,null,null,"X",null,"X",null,null,"9.12 (9.11/9.13)",null,5.3,9.1199999999999992,"https://asct-1.itrcweb.org/5-surface-geophysics/#5_3",null,null,"https://asct-1.itrcweb.org/9-12-gpr-data-show-location-of-buried-debris-and-piping-associated-with-a-former-gas-holder-in-minnesota/"]
["Multichannel Analysis of Surface Waves (MASW)","X",null,null,null,"X","X",null,null,"X","X",null,"X",null,null,"9.15 (9.14)",null,5.4,9.15,"https://asct-1.itrcweb.org/5-surface-geophysics/#5_4",null,null,"https://asct-1.itrcweb.org/9-15-surface-geophysical-methods-provide-data-to-identify-prospective-utility-waste-landfill-sites-in-karst-terrain-in-missouri/"]
["Seismic Reflection","X",null,null,null,"X","X",null,null,"X","X",null,"X",null,null,null,null,5.4,null,"https://asct-1.itrcweb.org/5-surface-geophysics/#5_4"]
["Seismic Refraction","X",null,null,null,"X","X",null,null,"X","X",null,"X",null,null,9.14,null,5.4,9.14,"https://asct-1.itrcweb.org/5-surface-geophysics/#5_4",null,null,"https://asct-1.itrcweb.org/9-14-seismic-refraction-electric-resistivity-and-multichannel-analysis-of-seismic-waves-provide-data-to-locate-monitoring-well-locations-in-a-mixed-use-area-in-northern-virginia/"]
["Frequency Domain Electromagnetics (FDEM)","X","X",null,null,"X","X",null,null,"X","X",null,"X",null,null,9.11,null,5.5,9.11,"https://asct-1.itrcweb.org/5-surface-geophysics/#5_5",null,null,"https://asct-1.itrcweb.org/9-11-surface-and-borehole-geophysical-technologies-provide-data-to-pinpoint-and-characterize-karst-features-at-a-former-retail-petroleum-facility-in-kentucky/"]
["Time Domain Electromagnetics (TDEM)","X","X","X",null,"X","X",null,"X","X","X",null,"X",null,null,9.16,null,5.5,9.16,"https://asct-1.itrcweb.org/5-surface-geophysics/#5_5",null,null,"https://asct-1.itrcweb.org/9-16-airborne-time-domain-electromagnetic-method-maps-sand-distribution-along-the-illinois-lake-michigan-shore/"]
["Remote Sensing",null,null,null,null,null,null,null,null,null,null,null,null,"RS_ST","RS_CL",null,null,6,null,"https://asct-1.itrcweb.org/6-remote-sensing/","https://asct-1.itrcweb.org/tables_checklists/asct_remote_sensing_rpas_summary_table.pdf","https://asct-1.itrcweb.org/tables_checklists/asct_remote_sensing_checklists.pdf"]
["Visual Spectrum Camera",null,null,null,"X",null,null,"X","X",null,"X",null,"X",null,null,"9.17 (9.18/9.19)",null,6.2,9.17,"https://asct-1.itrcweb.org/6-remote-sensing/#6_3",null,null,"https://asct-1.itrcweb.org/9-17-drone-technology-expedites-and-streamlines-site-characterization-at-a-former-golf-course-in-missouri/"]
["Multispectral Camera",null,null,"X",null,null,null,"X","X",null,"X",null,"X",null,null,"9.18 (9.17)",null,"6.4.1.11",9.17,"https://asct-1.itrcweb.org/6-remote-sensing/#6_4_1_11",null,null,"https://asct-1.itrcweb.org/9-18-high-resolution-and-thermal-aerial-images-identify-mine-openings-at-an-abandoned-colorado-mine/"]
["Hyperspectral Camera",null,null,"X",null,null,null,"X","X",null,"X",null,"X",null,null,null,null,"6.4.1.11",null,"https://asct-1.itrcweb.org/6-remote-sensing/#6_4_1_11"]
["Thermal/Long-Wave Infra-Red Camera","X","X","X",null,null,null,"X","X",null,"X",null,"X",null,null,"9.18 (9.17)",null,"6.4.1.12",9.17,"https://asct-1.itrcweb.org/6-remote-sensing/#6_4_1_12",null,null,"https://asct-1.itrcweb.org/9-18-high-resolution-and-thermal-aerial-images-identify-mine-openings-at-an-abandoned-colorado-mine/"]
["LiDAR",null,null,null,"X",null,null,"X","X",null,null,null,"X",null,null,null,null,"6.4.1.13",null,"https://asct-1.itrcweb.org/6-remote-sensing/#6_4_1_13"]
["Water Sampling",null,null,"X",null,null,null,"X","X",null,null,"X",null,null,null,null,null,6.6,9.19,"https://asct-1.itrcweb.org/6-remote-sensing/#6_6"]
["Air Sampling",null,null,"X",null,null,null,"X","X",null,null,"X",null,null,null,9.19,null,6.6,9.19,"https://asct-1.itrcweb.org/6-remote-sensing/#6_6",null,null,"https://asct-1.itrcweb.org/9-19-rpas-collects-water-samples-to-avoid-safety-concerns-at-montana-tunnels-mine/"]
[]
["X1 - these methods are typically direct-push, so may only be used in softer consolidated materials or in pre-drilled boreholes in bedrock."]
[]
["Category definitions/examples: "]
["Geology","Lithology, stratigraphy, fractures, structural, physical properties"]
["Hydrogeology","Porosity, permeability, flux, groundwater flow, hydraulic conductivity, hydraulic gradient"]
["Chemistry ","Chemical identification, NAPL presence, contaminant concentration, Parameter (pH, conductivity, organic content, total organic solids)"]
["Consolidated ","Can’t penetrate with push platforms"]
["Quantitative ","For chemistry – concentrations based on standards, for geo or hydro – parameter measurements that are generally repeatable"]
["Semi-quantitative","Measurements that fall within a range"]
["Qualitative","Chemistry - tool that provides an indirect measurement (LIF, PID); for geo or hydro –"]
[]
["Draft - November 30, 2019"]
[]
["Data Needed",null,null,"Subsurface",null,null,null,"Data Collection",null,null,null,"Data Quality"]
["All",null,null,"All",null,null,null,"All",null,null,null,"All"]
["Geology",null,null,"Consolidated /Bedrock  ",null,null,null,"Invasive",null,null,null,"Quantitative"]
["Hydrogeology",null,null,"Unconsolidated",null,null,null,"Non-Invasive",null,null,null,"Semi-Quantitative"]
["Chemistry",null,null,"Surface",null,null,null,null,null,null,null,"Qualitative"]
["Topography"]

{"sheet":"How to Use","index":1,"n_rows":29,"n_cols":4,"rows_kept":29,"cut":false,"hidden":false,"merged":[[2,1,2,11],[0,0,0,11],[1,0,1,11],[5,2,5,9],[3,1,3,11],[4,1,4,11],[11,3,11,11],[19,3,19,11],[6,3,6,11],[7,3,7,11],[8,3,8,11],[9,3,9,11],[10,2,10,11],[23,2,23,11],[12,3,12,11],[13,3,13,11],[15,3,15,11],[16,3,16,11],[14,2,14,11],[18,3,18,11],[17,2,17,11],[20,3,20,11],[21,1,21,11],[22,1,22,11],[24,2,24,11],[25,2,25,11],[26,2,26,11],[27,1,27,11],[28,1,28,11]]}
["ITRC Advanced Site Characterization Tools (ASCT) Selection Tool"]
["This Excel file includes the selection tool that helps a user to identify ASCT that may be appropriate for a site. The selection tool user is encouraged to visit the ITRC ASCT web page (http://pfas-1.itrcweb.org) to access the full Technical and Regulatory Guidance Document to which this spreadsheet provides support."]
["Step","Instructions"]
[1,"Considering ASCTs for use at a site includes evaluating tools in four general categories: direct sensing tools, borehole geophysical tools, surface geophysical tools, and remote sensing tools. "]
[2,"This selection tool allows a user to identify ASCT that may be appropriate for a site by selecting the evaluation criteria for the site. Using the pull-down boxes at the top of the selection tool, select the criteria applicable to the site. If all items of a particular criterion are required, select All. Choices for each criterion are provided below:"]
[null,null,"Data Needed - The type of data needed for the site"]
[null,null,null,"Chemistry  - chemical identification, NAPL presence, contaminant concentration, pH, conductivity, organic content, total organic solids"]
[null,null,null,"Geology - lithology, stratigraphy, fractures, structural, physical properties"]
[null,null,null,"Hydrology - porosity, permeability, flux, groundwater flow, hydraulic conductivity, hydraulic gradient"]
[null,null,null,"Topography - surface features"]
[null,null,"Subsurface/Surface - The type of subsurface or surface at the site"]
[null,null,null,"Consolidated/bedrock - consolidated soil or bedrock - subsurface soil likely cannot be penetrated with direct-push platforms"]
[null,null,null,"Unconsolidated - loosely arranged or unstratified soil, such as sand, silt, clay that are not cemented. Subsurface that can be penetrated by direct-push platforms"]
[null,null,null,"Surface - surface features such as surface cover, topography, sink holes, water bodies"]
[null,null,"Data Collection"]
[null,null,null,"Invasive - requires a boring or subsurface access"]
[null,null,null,"Non-invasive - access restrictions or other characteristics that restrict the installation of borings or access to the subsurface, or data collection related to surface cover, topology or other features that do not require borings or subsurface access"]
[null,null,"Data Quality"]
[null,null,null,"Quantitative - for chemistry – concentrations based on standards; for geo or hydro – parameter measurements that are generally repeatable"]
[null,null,null,"Semi-quantitative - measurements that fall within a range"]
[null,null,null,"Qualitative - an indirect measurement"]
[3,"Clicking the Search button will open a new sheet that lists the ASCT that match the selection criteria. "]
[4,"A short list of tools is on the new sheet listing the ASCT that match the selection criteria. Hyperlinks will be associated with each tool to link to additional information for each tool. Following the hyperlinks to the ASCT group section, individual tool sections, summary tables, case studies and checklists will provide you with the detailed information in the Technical and Regulatory Guidance Document for the short list of tools that match the selection criteria. "]
[null,null,"Links in Column A are to the Section in the ASCT document describing the tool or tool category"]
[null,null,"Links in Column O are to the Summary Table for the ASCT group"]
[null,null,"Links in Column P are to the Checklists for the ASCT group"]
[null,null,"Links in Column Q are to Case Studies for the ASCT"]
[5,"Returning to the Summary Table worksheet and repeating the selection process will result in multiple open worksheets."]
[6,"Saving a copy of the spreadsheet will retain the site-specific evaluation. Closing the spreadsheet without saving will discard your selections. "]

{"sheet":"Selection Tool","index":2,"n_rows":46,"n_cols":16,"rows_kept":46,"cut":false,"hidden":false,"merged":[[1,6,1,12],[6,13,6,15],[6,0,7,0],[6,11,6,12],[6,8,6,10],[6,5,6,7],[6,1,6,4]]}
[]
[null,null,null,null,null,null,"ITRC ASCT Selection Tool"]
[]
[]
[]
[]
["Tool","Data Needed",null,null,null,"Subsurface/Surface",null,null,"Data Quality",null,null,"Data Collection",null,"Additional Info"]
[null,"Geology","Hydrogeology","Chemistry","Topography","Consolidated /Bedrock  ","Unconsolidated","Surface","Quantitative","Semi-Quantitative","Qualitative","Invasive","Non-Invasive","Summary Table","Checklist","Case Study"]
["Direct Sensing",null,null,null,null,null,null,null,null,null,null,null,null,"DS_ST","DS_CL"]
["Membrane Interface Probe (MIP)",null,null,"X",null,"X1","X",null,null,"X",null,"X",null,null,null,"9.1 (9.2)"]
["Optical Image Profiler (OIP-UV, OIP-G)",null,null,"X",null,"X1","X",null,null,"X",null,"X",null,null,null,9.3000000000000007]
["Laser Induced Fluoresence (LIF)",null,null,"X",null,"X1","X",null,null,"X",null,"X",null,null,null,"9.4 (9.5/9.6)"]
["Cone Penetrometer Testing (CPT)","X","X",null,null,"X1","X",null,"X",null,null,"X",null,null,null,9.6999999999999993]
["Hydraulic Profiling (WaterlooAPS and HPT) ","X","X",null,null,"X1","X",null,"X","X","X","X",null,null,null,9.8000000000000007]
["Electrical Conductivity (EC)","X",null,"X",null,"X1","X",null,null,"X","X","X"]
["Flexible Underground Technology (FLUTe)",null,"X","X",null,"X",null,null,"X","X","X","X"]
["Borehole Geophysics",null,null,null,null,null,null,null,null,null,null,null,null,"BG_ST","BG_CL"]
["Fluid Temperature ",null,null,"X",null,null,null,null,"X",null,null,"X",null,null,null,9.9]
["Fluid Resisitivity",null,null,"X",null,"X",null,null,null,"X",null,"X",null,null,null,9.9]
["Mechanical Caliper ","X",null,null,null,"X",null,null,null,"X",null,"X",null,null,null,9.9]
["Optical Televiewer (OTV) ","X","X",null,null,"X",null,null,null,"X",null,"X",null,null,null,9.9]
["Acoustic Televiewer (ATV) ","X","X",null,null,"X",null,null,null,"X",null,"X",null,null,null,9.9]
["Natural Gamma ","X",null,null,null,"X","X",null,null,"X",null,"X",null,null,null,9.9]
["Heat Pulse Flow Meter",null,"X",null,null,null,null,null,null,"X",null,"X",null,null,null,9.9]
["Impeller Flowmeter","X","X",null,null,null,null,null,null,"X",null,"X"]
["Electrical Resitivity ",null,null,"X",null,"X",null,null,null,"X",null,"X",null,null,null,9.11]
["Nuclear Magnetic Resonance (NMR)",null,"X","X",null,"X","X",null,"X",null,null,"X",null,null,null,9.9]
["Borehole Video ","X",null,null,null,"X","X",null,null,null,"X","X",null,null,null,9.9]
["Surface Geophysics",null,null,null,null,null,null,null,null,null,null,null,null,"SG_ST","SG_CL"]
["Electrical Resistivity Inaging (ERI) (Tomography (ERT)) ","X","X","X",null,"X","X",null,null,"X","X",null,"X",null,null,"9.13 (9.10/9.15)"]
["Ground Penetrating Radar (GPR)","X","X",null,null,"X","X",null,null,null,"X",null,"X",null,null,"9.12 (9.11/9.13)"]
["Multichannel Analysis of Surface Waves (MASW)","X",null,null,null,"X","X",null,null,"X","X",null,"X",null,null,"9.15 (9.14)"]
["Seismic Reflection","X",null,null,null,"X","X",null,null,"X","X",null,"X"]
["Seismic Refraction","X",null,null,null,"X","X",null,null,"X","X",null,"X",null,null,9.14]
["Frequency Domain Electromagnetics (FDEM)","X","X",null,null,"X","X",null,null,"X","X",null,"X",null,null,9.11]
["Time Domain Electromagnetics (TDEM)","X","X","X",null,"X","X",null,"X","X","X",null,"X",null,null,9.16]
["Remote Sensing",null,null,null,null,null,null,null,null,null,null,null,null,"RS_ST","RS_CL"]
["Visual Spectrum Camera",null,null,null,"X",null,null,"X","X",null,"X",null,"X",null,null,"9.17 (9.18/9.19)"]
["Multispectral Camera",null,null,"X",null,null,null,"X","X",null,"X",null,"X",null,null,"9.18 (9.17)"]
["Hyperspectral Camera",null,null,"X",null,null,null,"X","X",null,"X",null,"X"]
["Thermal/Long-Wave Infra-Red Camera","X","X","X",null,null,null,"X","X",null,"X",null,"X",null,null,"9.18 (9.17)"]
["LiDAR",null,null,null,"X",null,null,"X","X",null,null,null,"X"]
["Water Sampling",null,null,"X",null,null,null,"X","X",null,null,"X"]
["Air Sampling",null,null,"X",null,null,null,"X","X",null,null,"X",null,null,null,9.19]
[]
["X1 - these methods are typically direct-push, so may only be used in softer consolidated materials or in pre-drilled boreholes in bedrock."]